COSHH assessment
	Company
	

	Task or process
	e.g. mixing two-part floor resin

	Location
	

	Assessed by
	

	Date
	

	Next review
	



1. The substance
	Product and supplier
	

	Safety data sheet date
	

	Form
	Liquid, powder, dust, fume, vapour, mist or gas

	Hazard statements
	From the label and section 2 of the data sheet

	Workplace exposure limit
	If any; see HSE's EH40/2005

	Amount used, and how often
	



2. Who could be exposed, and how
	Who
	Route (breathed in, skin, swallowed)
	How often and how long
	Notes

	Operators
	
	
	

	Maintenance and cleaning staff
	
	
	

	Contractors, visitors or the public
	
	
	



3. Controls, in order of priority
	Control
	In place now
	Further action
	Who
	By when

	Eliminate, or substitute something safer
	
	
	
	

	Use a safer form (e.g. paste, not powder)
	
	
	
	

	Change the process to release less
	
	
	
	

	Enclose the process
	
	
	
	

	Extract near the source (LEV)
	
	
	
	

	Keep as few people exposed as possible
	
	
	
	

	PPE that fits the wearer
	
	
	
	



4. Checks, monitoring and health surveillance
	LEV thorough examination and test
	At least every 14 months; last done:

	Exposure monitoring
	Needed? Why?

	Health surveillance
	Needed? What, how often, by whom

	Records of checks
	Where kept; keep for at least five years



5. Accidents and emergencies
☐  Spill kit and protective equipment for clearing up
☐  First aid steps from section 4 of the data sheet
☐  People trained to deal with a spill or a casualty
☐  Disposal of spill waste; information ready for the emergency services
6. Information and training
☐  Workers told the hazards, the controls and any exposure limit
☐  Trained to use the controls and PPE properly
☐  Told monitoring results and collective health surveillance results
☐  Contractors told the risks and controls
7. Review
	Date
	Reason for review
	Changes made
	By
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